**OVERSIZE OVERWEIGHT PERMIT**

*(Valid For One Power Unit Only)*

Permit No.

Permit Issued By: Pocahontas County Engineer’s Office

99 Court Square, Suite 4

Pocahontas, Iowa 50574-1629

Voice No.: (712)335-3252

Fax No.: (712)335-3282

|  |  |  |
| --- | --- | --- |
| Send To | Date | Fax Number |
| Address | | Will be invoiced for check or cash |
| Permit Type:  Single Trip ($35)  Round Trip ($70)  Annual Oversize ($50)  Annual Oversize/Overweight ($400)  Depending on the load, axle configuration and the bridges to be crossed, load capacity calculations may be required before the application can be approved or denied. The applicant will be required to pay the cost of these calculations even if the application is denied. The County will confirm that the applicant is aware of this extra cost before the information is sent to our structural consultant. | | |
| Valid Dates       to        ½ hour before sunrise to ½ hour after sunset  Continuous | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Requested By | | | | | | | Phone No. | | | | | | | | Issued By | | | | | | | |
| Issued To | | | | | | | | | | | | | | | | | | | | | | |
| Address | | | | | | | | | | | City / State / Zip | | | | | | | | | | | |
| Power Unit Year & Make | | | Power Unit License No. & State | | | | | | Power Unit Registered Weight | | | | Trailer Make | | | | | | | Trailer License No. & State | | |
| Object or Load | | | | | Model Number | | | | VIN | | | | | | | | | Serial Number | | | | SME Qualified |
| Overall Length | | Width | | Height | | Total Weight | | | | Trailer Length | | | | Load Length | | | | | Projections  Front       Rear | | | |
| Axle Weights | Single | | | Tandem | | | | Triple | | | | Quad | | | | Quint | | | | | Sextet | |
| Axle Spacing |  | | | | | | | | | | | | | | | | | | | | | |
| Trip From | | | | | | | | | | | Trip To | | | | | | | | | | | |
| Routes | | | | | | | | | | | | | | | | | | | | | | |
| GENERAL REQUIREMENTS  .  Civilian front Escort  With mounted height pole  Civilian rear escort  Amber revolving light/strobe  light with 360° visibility  Required on Highway        Required entire route  Law enforcement escort  Front Rear  See General Provisions for escort requirements for overwidth vehicles  Centerline all bridges at 5 mph.  Load must slow or stop when necessary to avoid approaching traffic when centerlining.  Round Trip. Return by reverse route with in same five days.  Run around clearance on route #        Run marked detour on route #  Signs and Flags must be displayed | | | | | | | | | | | | | | | | | Speed limit = Maximum posted limits unless otherwise specified on permit.  Must carry copy of permit and General Provisions dated 06/08 and comply with them.  Road must be clear of ice and snow and visibility must be at least ¼ mile.  Necessary city and/or state permits must be obtained separately.  Hazardous materials must be transported in compliance with applicable federal regulations. | | | | | |
| Special Requirement: | | | | | | | | | | | | | | | | | | | | | | |

Disclosure Statement: The information furnished on this application will be used by the Pocahontas Secondary Roads Department to prepare and issue permits. All information applicable to a given permit is required and is public information. Failure to complete the application as required will result in denial of permit. Permit issuing authorities will not be responsible for any damages that are the result of the move. Pocahontas County, the Secondary Road Department, and any other permit issuing authority assume no responsibility for the property of the permit holder.

Always check construction and weather conditions at www.511ia.org

